**Case No. 11-0944-EL-REN**

**Kenneth Martin Solar**

**Staff Interrogatories – Initial Set - Response**

Question 1:  Section G.4a of the application lists the Total PV Capacity (DC) as 16.640 kW. Section N.a lists the meter as an inverter meter. According to rule OAC 4901:1-40-04 (D)(1) facilities that are larger than 6 KW must measure output with a utility grade meter. Does the facility have an utility grade meter? If so please submit the photo (including date taken) and specifications of the utility grade meter.

Answer 1:

The meter that will be measuring the production reported to GATS is a utility grade meter not an inverter meter. The Manufacturer is GE and the Type is I-70-S.

